caruso.asc -- Digital signal of Caruso singing

Access
    Enrico = ReadSignal('Caruso');
  
Size
    50,000 by 1

Sampling Rate
    8192 Hz
    
Description
    In MATLAB, the command sound(Enrico,8192) will play this sound
    back at the right pitch.
    
Source
    Obtained by anonymous FTP from the xwplw package
    developed by R.R. Coifman and Fazal Majid at Yale University.
    You can get this X-windows adapted waveform analysis
    package by anonymous FTP to math.yale.edu.
